1. Sart the engine to build air pressure for the brake system.

2. Pump the service brake down until the air pressure is below 90 psi (governor kicks in)

3. Allow air pressure to build until governor kicks off at approximately 120 psi